#

##

##

    礦ision Build Log
    Project:
    E:\学习\全动电子液晶测试程序\液晶模块配套资料整理\新款资料制作\新款样品资料\3.97_IPS_OTM8009\STM32综合测试程序3.97寸OTM8009_800X480\USER\TOUCH.uvproj
    Project File Date:  12/31/2014

    Output:
    Load "..\\OBJ\\TOUCH.axf"
    Set JLink Project File to "E:\学习\全动电子液晶测试程序\液晶模块配套资料整理\新款资料制作\新款样品资料\3.97_IPS_OTM8009\STM32综合测试程序3.97寸OTM8009_800X480\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RB" selected (128 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.80g, compiled Feb 13 2014 20:50:02
    Firmware: J-Link ARM V8 compiled Nov 25 2013 19:20:08
    Hardware: V8.00
    S/N : 799713843
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFULL

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.293V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...