#

##

##

    礦ision Build Log
    Project:
    \\全动电子九楼服\e\工装测试程序\2.8寸LGDP4535工装测试程序带触摸_STM32Mini\USER\TOUCH.uvproj
    Project File Date:  02/27/2014

    Output:
    Build target 'Target 1'
    compiling main.c...
    main.c(45): warning:  #177-D: variable "i" was declared but never referenced
    main.c:   {     u16 i=0;
    main.c:             ^
    main.c: main.c: 1 warning, 0 errors
    compiling test.c...
    compiling GUI.c...
    linking...
    Program Size: Code=17270 RO-data=9226 RW-data=112 ZI-data=1648
    FromELF: creating hex file...
    "..\OBJ\TOUCH.axf" - 0 Error(s), 1 Warning(s).
    Load "..\\OBJ\\TOUCH.AXF"
    Set JLink Project File to "\\全动电子九楼服\e\工装测试程序\2.8寸LGDP4535工装测试程序带触摸_STM32Mini\USER\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.15n, compiled Jun 18 2010 19:55:09
    Firmware: J-Link ARM V8 compiled May 20 2010 17:07:46
    Hardware: V8.00
    S/N : 20100214
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.319V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Hardware-Breakpoints: 6
    Software-Breakpoints: 2048
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Application running ...
    Build target 'Target 1'
    compiling main.c...
    main.c(45): warning:  #177-D: variable "i" was declared but never referenced
    main.c:   {     u16 i=0;
    main.c:             ^
    main.c: main.c: 1 warning, 0 errors
    compiling test.c...
    compiling GUI.c...
    compiling lcd.c...
    compiling touch.c...
    linking...
    Program Size: Code=17262 RO-data=9226 RW-data=112 ZI-data=1648
    FromELF: creating hex file...
    "..\OBJ\TOUCH.axf" - 0 Error(s), 1 Warning(s).
    Load "..\\OBJ\\TOUCH.AXF"
    Set JLink Project File to "\\全动电子九楼服\e\工装测试程序\2.8寸LGDP4535工装测试程序带触摸_STM32Mini\USER\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.15n, compiled Jun 18 2010 19:55:09
    Firmware: J-Link ARM V8 compiled May 20 2010 17:07:46
    Hardware: V8.00
    S/N : 20100214
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.319V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Hardware-Breakpoints: 6
    Software-Breakpoints: 2048
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Application running ...
    Build target 'Target 1'
    compiling main.c...
    main.c(48): warning:  #223-D: function "KEY_Init" declared implicitly
    main.c:         KEY_Init();
    main.c:         ^
    main.c(45): warning:  #177-D: variable "i" was declared but never referenced
    main.c:   {     u16 i=0;
    main.c:             ^
    main.c: main.c: 2 warnings, 0 errors
    linking...
    Program Size: Code=17266 RO-data=9226 RW-data=112 ZI-data=1648
    FromELF: creating hex file...
    "..\OBJ\TOUCH.axf" - 0 Error(s), 2 Warning(s).
    Load "..\\OBJ\\TOUCH.AXF"
    Set JLink Project File to "\\全动电子九楼服\e\工装测试程序\2.8寸LGDP4535工装测试程序带触摸_STM32Mini\USER\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.15n, compiled Jun 18 2010 19:55:09
    Firmware: J-Link ARM V8 compiled May 20 2010 17:07:46
    Hardware: V8.00
    S/N : 20100214
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.319V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 0, TRES: 1, TRST: 0
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Hardware-Breakpoints: 6
    Software-Breakpoints: 2048
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Application running ...
    Build target 'Target 1'
    linking...
    Program Size: Code=17266 RO-data=9226 RW-data=112 ZI-data=1648
    FromELF: creating hex file...
    "..\OBJ\TOUCH.axf" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    compiling test.c...
    test.c(249): error:  #165: too few arguments in function call
    test.c:                 key=KEY_Scan();
    test.c:                              ^
    test.c: test.c: 0 warnings, 1 error
    compiling key.c...
    Target not created
    Build target 'Target 1'
    compiling test.c...
    linking...
    Program Size: Code=17334 RO-data=9226 RW-data=112 ZI-data=1648
    FromELF: creating hex file...
    "..\OBJ\TOUCH.axf" - 0 Error(s), 0 Warning(s).
    Load "..\\OBJ\\TOUCH.AXF"
    Set JLink Project File to "\\全动电子九楼服\e\工装测试程序\2.8寸LGDP4535工装测试程序带触摸_STM32Mini\USER\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.15n, compiled Jun 18 2010 19:55:09
    Firmware: J-Link ARM V8 compiled May 20 2010 17:07:46
    Hardware: V8.00
    S/N : 20100214
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.319V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Hardware-Breakpoints: 6
    Software-Breakpoints: 2048
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Application running ...
    Build target 'Target 1'
    compiling main.c...
    main.c(48): warning:  #223-D: function "KEY_Init" declared implicitly
    main.c:         KEY_Init();
    main.c:         ^
    main.c(45): warning:  #177-D: variable "i" was declared but never referenced
    main.c:   {     u16 i=0;
    main.c:             ^
    main.c: main.c: 2 warnings, 0 errors
    compiling test.c...
    compiling GUI.c...
    compiling lcd.c...
    compiling touch.c...
    linking...
    Program Size: Code=17334 RO-data=9226 RW-data=112 ZI-data=1648
    FromELF: creating hex file...
    "..\OBJ\TOUCH.axf" - 0 Error(s), 2 Warning(s).
    Build target 'Target 1'
    compiling lcd.c...
    linking...
    Program Size: Code=17342 RO-data=9226 RW-data=112 ZI-data=1648
    FromELF: creating hex file...
    "..\OBJ\TOUCH.axf" - 0 Error(s), 0 Warning(s).
    Load "..\\OBJ\\TOUCH.AXF"
    Set JLink Project File to "\\全动电子九楼服\e\工装测试程序\2.8寸LGDP4535工装测试程序带触摸_STM32Mini\USER\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.15n, compiled Jun 18 2010 19:55:09
    Firmware: J-Link ARM V8 compiled May 20 2010 17:07:46
    Hardware: V8.00
    S/N : 20100214
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.319V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Hardware-Breakpoints: 6
    Software-Breakpoints: 2048
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Application running ...
    Build target 'Target 1'
    compiling lcd.c...
    linking...
    Program Size: Code=17342 RO-data=9226 RW-data=112 ZI-data=1648
    FromELF: creating hex file...
    "..\OBJ\TOUCH.axf" - 0 Error(s), 0 Warning(s).
    Load "..\\OBJ\\TOUCH.AXF"
    Set JLink Project File to "\\全动电子九楼服\e\工装测试程序\2.8寸LGDP4535工装测试程序带触摸_STM32Mini\USER\JLinkSettings.ini"

    JLink info:
    ------------
    DLL: V4.15n, compiled Jun 18 2010 19:55:09
    Firmware: J-Link ARM V8 compiled May 20 2010 17:07:46
    Hardware: V8.00
    S/N : 20100214
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RB
    VTarget = 3.319V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 0, TMS: 0, TRES: 1, TRST: 0
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Hardware-Breakpoints: 6
    Software-Breakpoints: 2048
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    * JLink Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Application running ...
    Build target 'Target 1'
    compiling lcd.c...
    linking...
    Program Size: Code=17342 RO-data=9226 RW-data=112 ZI-data=1648
    FromELF: creating hex file...
    "..\OBJ\TOUCH.axf" - 0 Error(s), 0 Warning(s).